**FILTER**

**PRESOAK and RINSE PROCEDURE**

1. Prepare 50:50 v/v isopropanaol:water in a large beaker
2. Place and immerse completely new filter in solution
3. Allow to presoak at least overnight
4. Place filter rinse apparatus in sink
5. Firmly attached presoaked filter in filter apparatus
6. Connect water hose to DI water
7. Turn on DI water flow
8. Allow to rinse for 30-60 minutes. Ensure that isopropanol is completely rinsed out
9. Leave filter in beaker filled DI water only until ready to install on tool