**ClassOne Semitool SRD Power Up Procedure**

**Equipment Location:** 6-019

**Authorized Employees:** Adele Pacquette, Christopher Guarino

**Manager:** Eugene O’Sullivan (x3997)

**Equipment:** ClassOne Semitool SRD

**BT/ID Number:** ClassOne ID: 3805

**Procedure:**

1. If Closed, Open the DI Water and Nitrogen gas valves.
   1. On the wall to the left of the tool.
2. Flip toggle-switch ‘Power’ to the ‘On’ position.
   1. When the display reads ‘IDLE’ initialization is complete.
3. Notify a tool operator that the tool has been powered on.
4. It is the responsibility of the tool operator to note the position of any wafers in the tool and recover the wafers.