**Eeja RAD-Plater Power Up Procedure**

**Equipment Location:** 1-130

**Authorized Employees:** Adele Pacquette, Christopher Guarino

**Manager:** Eugene O’Sullivan (x3997)

**Equipment:** Eeja RAD-Plater

**BT/ID Number:**

**Procedure:**

1. If Off, turn On the Power Breaker on the wall to the right of the tool.
   1. Confirm that the ‘Main Power On’ light is lit.
2. If Closed, Open the Compressed Air and Nitrogen gas valves.
   1. On the wall to the right of the tool.
3. If Closed, Open the blue OFA valve (Compressed Air).
4. Notify a tool operator that the tool has been powered on.
5. It is the responsibility of the tool operator to note the position of any wafers in the tool and recover the wafers.