**KLA Tencor P-11 Profiler Power Up Procedure**

**Equipment Location:** 1-150

**Authorized Employees:** Michael Lofaro, Andrew Giannetta, Joseph Bauer, Michael Chido, Christopher Guarino, Ricky Hull, Ravi Patel

**Manager:** Eugene O’Sullivan (x3997)

**Equipment:** KLA Tencor Profiler

**BT/ID Number:** 824700B

**Procedure:**

1. Power on the computer.
2. After Start-Up, double click ‘Profiler’ short-cut on the ‘Program Manager Screen’.
3. Double click ‘Scan’ on the ‘Top Level Menu’ screen.
4. Select the appropriate recipe.
   1. Typically recipe ‘CJ2D’.
5. Click ‘XY View’ at the bottom right of the screen.
6. Notify a tool operator that the tool has been powered on.
7. It is the responsibility of the tool operator to note the position of any wafers in the tool and recover the wafers.