**KLA Tencor OmniMap RS75 Power Up Procedure**

**Equipment Location:** 6-019

**Authorized Employees:** Adele Pacquette, Christopher Guarino

**Manager:** Eugene O’Sullivan (x3997)

**Equipment:** KLA Tencor OmniMap RS75

**BT/ID Number:** 2 MGNE 0010015992

**Procedure:**

1. Open door on computer and press the ‘Power’ button.
   1. The software initializes on start-up. May take a few minutes to be operational.
2. Press the green ‘On’ button on the front of the tool.
3. Notify a tool operator that the tool has been powered on.
4. It is the responsibility of the tool operator to note the position of any wafers in the tool and recover the wafers.