MicroSense

Chris Guarino Living Notes

Operations Procedure

Steps:

1. Turn ON.
2. Open UltraMap software.
3. Start / Measurement
4. Select proper recipe.
   1. It will likely always be “DIAMETER SCAN 95MM EXCL”
5. Click Measure Tab.
6. Enter LOT name in the top with process in the top.
7. Enter wafer numbers in the bottom right.
   1. You have too ADD each one manually.
8. No hit Start.
   1. The software will prompt you to unload and load each wafer.
      1. To be sure that vacuum is operating properly check the “Stage Vacuum On” box before starting. You should hear a click.
9. Record Results

Record Results:

Ex:

|  |  |  |  |
| --- | --- | --- | --- |
| Wafer | Mean | Min | Max |
| # |  |  |  |

Notes:

* At the beginning of the week you must run a qualifying wafer.
  + It is under the machine. Spreadsheet is on the desktop. IBM\_21 Point Recipe