**ClassOne Solstice Plater Power Up Procedure**

**Equipment Location:** 6-019

**Authorized Employees:** Adele Pacquette, Christopher Guarino

**Manager:** Eugene O’Sullivan (x3997)

**Equipment:** ClassOne Solstice Damascene Plater

**BT/ID Number:**

**Procedure:**

1. Press the Green ‘On’ button on the left side of the tool.
   1. This will initialize the tool’s systems and computer.
2. Software will initialize upon start-up.
3. Once software is fully loaded, click ‘Login’ in the top right of the screen.
   1. Note that you can not interact with the software until you login.
4. Enter, Username: Engineer, Password: c1t
   1. Case-sensitive.
5. Notify a tool operator that the tool has been powered on.
6. It is the responsibility of the tool operator to note the position of any wafers in the tool and recover the wafers.