**Ebara FREX200 Polisher Power Up Procedure**

**Equipment Location:** 6-043

**Authorized Employees:** Michael Lofaro, Andrew Giannetta, Joseph Bauer, Michael Chido, Chris Guarino

**Manager:** Eugene O’Sullivan (x3997)

**Equipment:** Ebara FREX200 Polisher

**BT/ID Number:** 2 MGNE 0010045170

**Procedure:**

1. Press the “On” button on the front panel. Power up will take ~5-10 minutes.
2. If an alarm sounds during power up, press the “Buzzer Reset” button (which should be lit). **Do not attempt to reset the fault.**
3. Notify a tool operator that the tool has been powered on.
4. It is the responsibility of the tool operator to note the position of any wafers in the tool and recover the wafers.