**ECI QualiLab Plating Bath Analyzer Power Up Procedure**

**Equipment Location:** 6-019

**Authorized Employees:** Adele Pacquette, Christopher Guarino

**Manager:** Eugene O’Sullivan (x3997)

**Equipment:** ECI QualiLab Plating Bath Analyzer

**BT/ID Number:** MGNE 0010104726

**Procedure:**

1. Flip toggle-switch ‘Power’ to the ‘On’ position.
   1. This will initialize the computer.
2. On screen, select ‘Start Windows Normally’.
3. Double click QualiLab 6.3.1 short-cut.
4. Enter, Username: Engineer, Password: 2
   1. Tool software initializes.
5. Notify a tool operator that the tool has been powered on.
6. It is the responsibility of the tool operator to note the position of any wafers in the tool and recover the wafers.