**CDE ResMap Power Up Procedure**

**Equipment Location:** 1-150

**Authorized Employees:** Michael Lofaro, Andrew Giannetta, Joseph Bauer, Michael Chido, Christopher Guarino, Ricky Hull, Ravi Patel

**Manager:** Eugene O’Sullivan (x3997)

**Equipment:** CDE ResMap

**BT/ID Number:** 2 MGNE 0010128916

**Procedure:**

1. Flip toggle-switch to the ‘On’ position on the right side of the tool.
2. Power on the computer.
   1. Tool software will initialize on start-up.
3. Notify a tool operator that the tool has been powered on.
4. It is the responsibility of the tool operator to note the position of any wafers in the tool and recover the wafers.