**OnTrak Brush Cleaner Power Up Procedure**

**Equipment Location:** 1-138 / 1-110

**Authorized Employees:** Andrew Giannetta, Mike Lofaro, Joseph Bauer, Michael Chido, Christopher Guarino, Ricky Hull, Ravi Patel

**Manager:** Eugene O’Sullivan (x3997)

**Equipment:** OnTrak Brush Cleaner

**BT/ID Number:** 10120 / 10225

**Procedure:**

1. Press the “On” button on the front panel. Power up will take ~5-10 minutes.
2. If an alarm sounds during power up, press the “Yellow Light Bulb” button on the lower right of the touch screen (which should be lit). **Do not attempt to reset the fault.**
3. Notify a tool operator that the tool has been powered on.
4. It is the responsibility of the tool operator to note the position of any wafers in the tool and recover the wafers.